# disable

#### Syntax

To return to User Exec mode:

disable [ level ]

For DVMRP, RIP:

[ no ] disable

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

When used from Privileged Exec mode, exits Privileged Exec mode and returns to User Exec mode.

When used from Router Configuration or Interface Configuration mode in the context of a DVMRP configuration, disables DVMRP on the virtual router or interface. The no version reenables DVMRP on the virtual router or interface.

When used from Router Configuration mode in the context of a RIP configuration, disables RIP on the virtual router. The no version enables RIP processing on the virtual router.

#### Options

- level—One of the following privilege levels; default value is 1
  - 0—Allows the user to execute the help, enable, disable, and exit commands
  - 1—Allows the user to execute commands in User Exec mode plus commands at level 0
  - 5—Allows the user to execute Privileged Exec show commands plus the commands at levels 1 and 0
  - 10—Allows the user to execute all commands except support commands, which may be provided by Juniper Networks Customer Service
  - 15—Allows the user to execute support commands

#### Mode

Address Family Configuration (RIP), Interface Configuration (DVMRP only), Privileged Exec, Router Configuration (DVMRP or RIP)