# show ipv6 pim interface

#### Syntax

show ipv6 pim interface
{ summary | [ interfaceType interfaceSpecifier ] [ detail | count ] [ filter ] }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays information about each PIM IPv6 interface.

#### Options

- summary—Displays the number of configured, enabled, and disabled PIM sparse mode interfaces
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- detail—Displays detailed information for all PIM interfaces or for a specified PIM interface
- count—Displays the number of incoming and outgoing PIM control packets
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec