# show atm vp-description

#### Syntax

show atm vp-description [ interfaceSpecifier [ vpi ] ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays descriptions configured for virtual paths (VPs) on an ATM interface. You can display all VP descriptions configured on the router, all VP descriptions configured for a particular interface, or the VP description configured for a particular VPI.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- vpi—Virtual path identifier number, in the range 0–255
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec