# ipv6 mld group limit

#### Syntax

ipv6 mld group limit groupLimit

no ipv6 mld group limit

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Limits the number of MLD groups that an interface can accept. The no version restores the default situation, in which there is no limit to the number of MLD groups that the interface accepts.

#### Options

- groupLimit—Maximum number of MLD groups that an interface can accept, in the range 0–64,000

#### Mode

Interface Configuration, Profile Configuration