# ipv6General

#### Description

IPv6 general

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

License-related errors (for example, attempting to configure IPv6 without configuring the license first); error in sending interface up or down events to IPv6

#### Warning Log

Primary IPv6 address on an interface is not found

#### Notice Log

None

#### Info

None

#### Debug

None

#### Filter 1

interface interfaceType interfaceSpecifier

- interface—Logs events for a specific interface
- interfaceType—Type of interface for which you want to log events
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JunosE Command Reference Guide.

#### Filter 2

router virtualRouterName [ interface interfaceType interfaceSpecifier ]

- router—Logs events for a specific virtual router
- virtualRouterName—Name of virtual router for which you want to log events
- interface—Logs events on a specific interface on the virtual router
- interfaceType—Type of interface for which you want to log events (for example, atm or fastEthernet)
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JunosE Command Reference Guide.