# exit-address-family

#### Syntax

exit-address-family

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Exits from Address Family Configuration mode and returns to Router Configuration mode. There is no no version.

#### Mode

Address Family Configuration

#### Related Documentation

- Configuring BGP Signaling for L2VPNs and Configuring BGP Signaling for VPLS in the JunosE BGP and MPLS Configuration Guide