# mpls ldp targeted-hello send list

#### Syntax

[ no ] mpls ldp targeted-hello send list
{ access-list accessListName | ipAddress [ ipAddress ]* }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the list of peer addresses to which MPLS sends targeted hello messages and from which MPLS accepts targeted hello messages. The no version removes the list of peer addresses.

#### Options

- accessListName—String of up to 32 alphanumeric characters that identifies an access list
- ipAddress—IP address of a peer
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Global Configuration