# mpls ldp profile

#### Syntax

In Global Configuration mode:

mpls ldp [ interface ] profile [ profileName ]

no mpls ldp interface profile profileName

In Interface Configuration mode:

mpls ldp profile profileName

no mpls ldp profile

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

In Global Configuration mode, creates or modifies a configuration profile for LDP. Places the CLI in LDP Configuration mode. The implicit default LDP profile specifies a value of 0 for hello hold-time; this value signifies 15 seconds for link hellos and 45 seconds for targeted hello messages.

Any change to a profile affects all interfaces that use the profile; changes are effective the next time the interface comes up.

In Interface Configuration mode, creates or enables LDP on the interface with the factory default profile or the specified profile. The no version reverts to the default profile on the interface.

In both modes, if you specify a profile not previously configured, it is created with the factory default settings. If you do not specify a profile name, the factory default profile is assumed. The no version deletes the specified profile.

#### Options

- interface—Keyword required for the no version in Global Configuration mode
- profileName—Name of a profile to be created or modified (Global Configuration mode), applied to an interface (Interface Configuration mode), or deleted (both modes); the profile sets the values for the protocol parameters; until you modify the profile settings, the values match those of the implicit default profile

#### Mode

Global Configuration, Interface Configuration