# router ospf

#### Syntax

[ no ] router ospf processId [ vrf vrfName ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures an OSPF routing process. The no version disables an OSPF routing process.

#### Options

- processId—Number, in the range 1–65535, that identifies the OSPF process
- vrfName—Name of the VRF; string of 1–32 alphanumeric characters; available only in virtual router context, not VRF context

#### Mode

Global Configuration

#### Related Documentation

- Configuring Routing in the Core for VPLS in the JunosE BGP and MPLS Configuration Guide