# clear ip routes download

#### Syntax

For a specific VRF

clear ip routes download [ vrf vrfName ] { ipAddress ipMask | * }

For all virtual routers

clear ip routes download { all | reload }

#### Release Information

Command introduced in JunosE Release 8.1.0.

#### Description

Synchronizes downloaded access routes and the routes installed in the routing table. This command has no effect if a download operation is in progress. There is no no version.

#### Options

- vrfName—Name of the VRF; string of 1–32 alphanumeric characters; the current virtual router is used by default
- ipAddress—IP address prefix to clear
- ipMask—Network mask of the IP address prefix to clear
- *—Clears all dynamic routes that are installed in the routing table of the current virtual router or specified VRF
- all—Clears all downloaded routes that are installed in the routing tables of all virtual routers and VRFs.
- reload—Performs a route download operation, then clears all downloaded routes from the routing tables in all virtual routers and VRFs.

#### Mode

Privileged Exec