# mdt-interval

#### Syntax

mdt-interval time

no mdt-interval

#### Release Information

Command introduced in JunosE Release 8.2.0.

#### Description

Configures the time in seconds between successive MLD join TLVs. The no version returns to the default.

#### Options

- time—Time between successive MLD join TLV in the range 1–300 seconds; the default is 60

#### Mode

IP PIM Data MDT Configuration