# mpls ldp targeted-hello interval

#### Syntax

mpls ldp targeted-hello interval seconds

no mpls ldp targeted-hello interval

#### Release Information

Command introduced in JunosE Release 8.1.0.

#### Description

Configures the the interval between targeted hello packets sent by LDP. This command takes effect immediately. The no version restores the default value, 15 seconds.

#### Options

- seconds—Number of seconds, in the range 1–65535

#### Mode

Global Configuration