# show atm bulk-config

#### Syntax

show atm bulk-config [ atm interfaceSpecifier ] [name bulkConfigName ] [ override ]
[ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays information, including base profile assignments and overriding profile assignments, for the bulk-configured VC ranges on an ATM AAL5 interface. You can display information for all VC ranges on the router, for all VC ranges on a particular ATM AAL5 interface, or for the VC range associated with a particular bulk configuration name.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- bulkConfigName—Name associated with a VC range on the ATM AAL5 interface, as specified in the atm bulk-config command
- override—Displays information only about each overriding profile assignment configured for a specific ATM PVC within a bulk-configured VC subrange; when you use the override keyword, information about base profile assignments is not displayed
- filter—SeeFiltering show Commands

#### Mode

Privileged Exec, User Exec