# show ipsec transport interface

#### Syntax

show ipsec transport interface [ detail ] [ application applicationType ]
[ state { up | down } ] [ interfaceName |
[ virtual-router vrName ] destination destAddress | local localAddress ] [ filter ]

To display summary information:

show ipsec transport interface summary

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays all details, including statistics, of IPSec transport connections that match the specified criteria.

#### Options

- detail—Includes statistics for the displayed connection
- applicationType—Application protected by IPSec transport connections
- state—Displays connections that are in the specified state, up or down
- interfaceName—Connection number that you want to display
- vrName—Name of a virtual router. If you do not specify a virtual router, the router displays connections on the current virtual router context. Notice that the local and destination IP addresses exist in the current virtual router context.
- destAddress—IP address of remote endpoint
- localAddress—IP address of local endpoint
- filter—See Filtering show Commands
- summary—Displays a summary of all IPSec transport connections

#### Mode

Privileged Exec