# radiusSendAttributes

#### Description

RADIUS attributes added to Access-Accept (inbound RADIUS requests), Acct-Start, Interim-Acct, and Acct-Stop messages

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

None

#### Notice Log

None

#### Info

Parse errors that occur in L2C and DSL Forum attribute strings

#### Debug

Attributes that are added to outbound RADIUS requests, including Access-Request, Acct-Start, Acct-Stop, interim accounting requests, tunnel accounting requests, and ICR partition accounting requests; IPv6 accounting VSA attributes (IPv6-Acct-Input-Octets [26-151], IPv6-Acct-Output-Octets [26-152], IPv6-Acct-Input-Packets [26-153], IPv6-Acct-Output-Packets [26-154], IPv6-Acct-Input-Gigawords [26-155], and IPv6-Acct-Output-Gigawords [26-156]) that are added to outbound RADIUS requests, including Acct-Stop and interim accounting requests; IPv6 RADIUS IETF and VSA attributes (Ipv6-NdRa-Prefix [26-129], Ipv6-Virtual-Router [26-45], Ipv6-Local-Interface [26-46], Ipv6-Primary-DNS [26-47], Ipv6-Secondary-DNS [26-48], Framed-IPv6-Route [99], Framed-IPv6-Pool [100], Delegated-Ipv6-Prefix [123]) that are added to Access-Accept (inbound RADIUS requests), Acct-Start, Interim-Acct, and Acct-Stop messages; DHCP Option 82 [26–159] which is added to trigger packet mirroring for DHCP subscribers; failed to configure radiusPerProfileMap entry due to the unavailability of the resource, insertion failure, and no such entry; restore radiusPerProfileMap due to map insertion failure

#### Filter

None