# show mpls fast-reroute database

#### Syntax

show mpls [ traffic-eng ] fast-reroute database [ ipAddress ]
[ name tunnelName ] [ interface interfaceType interfaceSpecifier ]
[ status { all | desired | establishing | established | active | unknown } ]
[ count-only ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays information about the backup state of protected primary tunnels.

#### Options

- traffic-eng—Specifies optional keyword for compatibility with non–E Series implementations
- ipAddress—Address of the endpoint for the primary LSP; meaningful only for the tunnel ingress node
- tunnelName—Name of the primary LSP; meaningful only for the tunnel ingress node
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- status—Displays only entries with the specified status:
  - all—Displays all entries regardless of backup protection status
  - desired—Displays entries where backup protection is desired
  - establishing—Displays entries where backup protection is being established
  - established—Displays entries where backup protection is established
  - active—Displays entries where backup protection is active
  - unknown—Displays entries where status of backup protection is unknown
- count-only—Displays count of entries matching command specification
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec