# set ip interface-profile

#### Syntax

set ip interface-profile profileName

no set ip interface-profile

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies a dynamic IP interface profile that is used in the route map. The no version removes the interface profile from the route map.

#### Options

- profileName—Name of the dynamic profile

#### Mode

Route Map Configuration