# Monitoring AAA Domain Name Stripping for a Domain Per Virtual Router

#### Purpose

Display information about the aaa domain-name stripping functionality per virtual router.

#### Action

To display information about the aaa domain-name stripping functionality per virtual router:

    host1:vr1(config)#show aaa strip-domain

    strip-domain is disable

    strip-domain domainName delimiter is “@”

    strip-domain domainName parse direction is right-to-left

#### Meaning

Table 14 lists the show aaa strip-domain command output fields.

Table 14: show aaa strip-domain Output Fields

Field Name | Field Description
--- | ---
delimiter | Delimiter value configured for the subscriber’s domain
domainName | The domain name characteristics configured for the broadband remote access subscriber per virtual router
disable | The domain name stripping functionality is disabled for the virtual router
enable | The domain name stripping functionality is enabled for the virtual router
left-to-right | The parsing direction configured for stripping the domain name at the virtual router is left-to-right
right-to-left | The parsing direction configured for stripping the domain name at the virtual router is right-to-left

#### Related Documentation

- show aaa delimiters
- show aaa strip-domain
- aaa domain-map
- ppp authentication