# bulkstats schema subtree qos

#### Syntax

bulkstats schema schemaIndex subtree qos [ subtreelist qosList [ qosList ]*| export-summarized-stats ]

no bulkstats schema schemaIndex

#### Release Information

Command introduced in JunosE Release 11.1.0.

#### Description

Configures the bulk statistics schema to collect QoS statistics and configuration information on egress queues belonging to different interface types. The no version removes the schema.

#### Options

- schemaIndex—Identifier for the schema in the range 1–65535
- qosList—Select one of the following queue attributes:
  - aggregate-drop-rate—Configures QoS schema to export the average drop rate within the rate-period specified in the statistics profile of the egress queue
  - all—Configures QoS schema to export all statistics; this is the default option
  - assured-rate—Configures QoS schema to export the assured rate attribute
  - burst—Configures QoS schema to export the burst attribute
  - byte-adjustment-bytes—Configures QoS schema to export the number of bytes configured for the byte-adjustment application, if the byte-adjustment application is enabled on the queue
  - byte-adjustment-type—Configures QoS schema to export the type of byte-adjustment , if byte-adjustment application is enabled on the queue
  - drop-profile—Configures QoS schema to export the drop profile name associated with the queue
  - forwarded-bytes—Configures QoS schema to export the number of bytes forwarded from the queue
  - forwarded-packets—Configures QoS schema to export the number of forwarded packets from the queue
  - forwarded-rate—Configures QoS schema to export the average forwarded rate within the rate period specified on the statistics profile of the queue
  - green-dropped-bytes—Configures QoS schema to export the number of bytes of green traffic that was dropped on this queue
  - green-dropped-packets—Configures QoS schema to export the number of packets of green traffic that was dropped on this queue
  - parent-shaping-rate—Configures QoS schema to export the shaping rate enabled on the parent interface in the scheduling hierarchy
  - parent-shared-shaping-rate—Configures QoS schema to export the shared shaping rate enabled on the parent interface in the scheduling hierarchy
  - parent-weight—Configures QoS schema to export the aggregate weight of the parent interface
  - queue-length—Configures QoS schema to export the queue length attribute
  - queue-profile—Configures QoS schema to export the queue profile name
  - red-dropped-bytes—Configures QoS schema to export the number of bytes of red traffic that was dropped on the queue
  - red-dropped-packets—Configures QoS schema to export the number of red packets that was dropped on the queue
  - RED-enabled—Configures QoS schema to verify whether the Random Early Detect (RED) option is enabled on the queue
  - scheduler-profile—Configures QoS schema to export the scheduler profile name
  - shaping-mode—Configures QoS schema to export the shaping mode attribute
  - shaping-rate—Configures QoS schema to export the shaping rate attribute
  - shared-shaping-mode—Configures QoS schema to export the shared shaping mode attribute
  - shared-shaping-rate—Configures QoS schema to export the shared shaping rate attribute
  - statistics-profile—Configures QoS schema to export the statistics profile name
  - weight—Configures QoS schema to export the weight assigned to the queue
  - yellow-dropped-bytes—Configures QoS schema to export the number of bytes of yellow traffic that was dropped on the queue
  - yellow-dropped-packets—Configures QoS schema to export the number of yellow packets that were dropped on the queue
- export-summarized-stats—Exports the summarized QoS rate statistics over each S-VLAN or ATM VP (virtual path)
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Global Configuration

#### Related Documentation

- Configuring SNMP in JunosE System Basics Configuration Guide
- QoS Statistics Overview