# rsvpInterface

#### Description

RSVP interface

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Setup errors; operational errors; invalid configuration errors

#### Warning Log

Nonfatal allocation errors

#### Notice Log

None

#### Info

Minor internal errors

#### Debug

Function flows

#### Filter

router virtualRouterName [ interface interfaceType interfaceSpecifier ]

- router—Logs events for a specific virtual router
- virtualRouterName—Name of virtual router for which you want to log events
- interface—Logs events on a specific interface on the virtual router
- interfaceType—Type of interface for which you want to log events
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JunosE Command Reference Guide.