# Monitoring Prefix List Outbound Route Filters Received from the BGP Neighbor

#### Purpose

Display prefix-list outbound route filters received from the BGP neighbor.

#### Action

To display prefix-list outbound route filters received from the specified neighbor:

    host1#show ip bgp neighbors 192.168.1.158 received prefix-filter
    ip prefix-list filter 192.168.1.158 for address family ipv4:unicast
       seq 5 permit 10.1.1.1/32
       seq 10 permit 10.1.1.2/32
       seq 15 permit 10.1.1.3/32

#### Meaning

Table 38 lists the show ip bgp neighbors received prefix-filter command output fields.

Table 38: show ip bgp neighbors received prefix-filter

Field Name | Field Description
--- | ---
seq | Sequence number of the entry in the prefix list
permit, deny | Condition statement for addresses matching the listed address

#### Related Documentation

- show ip bgp neighbors