# tcp resequence-buffers default-connection-maximum

#### Syntax

[ ip ] tcp resequence-buffers default-connection-maximum defaultConnMaxValue

no [ ip ] tcp resequence-buffers default-connection-maximum

#### Release Information

Command introduced before JunosE Release 7.1.0.
ip keyword made optional in JunosE Release 7.2.0.

#### Description

Specifies the default buffer limit assigned to all TCP connections on a virtual router unless a specific limit is set for the VR in which the connection is established. Specifying a value of zero (0) buffers turns off the default limit. The no version reverts the connection maximum value to its default (10 buffers).

#### Options

- ip—Optional keyword for use with older scripts
- defaultConnMaxValue—Default number of maximum buffers for newly created connections on a virtual router, in the range 1–65535

#### Mode

Global Configuration