# ip pim join-filter

#### Syntax

ip pim join-filter accessListName

no ip pim join-filter

#### Release Information

Command introduced before JunosE Release 7.1.0.
Profile Configuration mode added in JunosE Release 8.2.0.

#### Description

Specifies an extended access list that you want this PIM interface to use as a join filter. If an interface-level filter exists, it takes precedence over the global-level filter. The no version removes the filter association.

#### Options

- accessListName—Name of the access list that you want this interface to use as a PIM join filter; a string of up to 32 alphanumeric characters

#### Mode

Global Configuration, Interface Configuration, Profile Configuration