# equipment loopback

#### Syntax

equipment { customer | network } loopback

no equipment

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables or disables the router's ability to be placed in loopback by a remote device connected on a CT3 or T3 interface. The no version disables the router's ability to be placed in loopback by the remote device.

#### Options

- customer—Enables the router to enter into loopback when it receives an appropriate signal from the remote interface
- network—Disables the router's ability to enter into loopback when it receives an appropriate signal from the remote interface

#### Mode

Controller Configuration