# l2tp classifier-list

#### Syntax

l2tp classifier-list classifierName [ traffic-class trafficClassName ]
[ color { green | yellow | red } ] [ user-packet-class userPacketClassValue ]

no l2tp classifier-list classifierName [ classifierNumber ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Creates or modifies a classifier control list. The no version removes the classifier control list.

#### Options

- classifierName—Name of the classifier control list entry
- classifierNumber—Index of the classifier list entry; use the show classifier-list command to see a list of entries with index numbers
- trafficClassName—Name of the traffic class to match
- green—Matches packet color to green, indicating a low drop preference
- yellow—Matches packet color to yellow, indicating a medium drop preference
- red—Matches packet color to red, indicating a high drop preference
- userPacketClassValue—User packet class value

#### Mode

Global Configuration

#### Related Documentation

- Creating or Modifying Classifier Control Lists for L2TP Policy Lists