# neighbor soft-reconfiguration inbound

#### Syntax

[ no | default ] neighbor { ipAddress | ipv6Address | peerGroupName }
soft-reconfiguration inbound

#### Release Information

Command introduced before JunosE Release 7.1.0.
ipv6Address variable added in JunosE Release 8.0.0.

#### Description

Initiates storage of unmodified copies of routes from the specified neighbor or all members of the specified peer group. The no version halts this storage. The default version removes the explicit configuration from the peer or peer group and reestablishes inheritance of the feature configuration.

#### Options

- ipAddress—IP address of BGP neighbor
- ipv6Address—IPv6 address of BGP neighbor
- peerGroupName—Name of a BGP peer group. If you specify a BGP peer group by using the peerGroupName argument, all the members of the peer group inherit the characteristic configured with this command, unless it is overridden for a specific peer.

#### Mode

Address Family Configuration, Router Configuration