# multicastTraffic

#### Description

IP multicast frame transmit or receive

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

None

#### Notice Log

None

#### Info

None

#### Debug

IP multicast packet transmit or receive information

#### Filter 1

remote-ip-address ipAddress [ ipAddressMask ]

- remote-ip-address—Logs events for a remote address
- ipAddress—Address of remote system for which you want to log messages
- ipAddressMask—Mask for the remote address

#### Filter 2

router virtualRouterName [ remote-ip-address ipAddress [ ipAddressMask ] ]

- router—Logs events on a specific virtual router
- virtualRouterName—Name of virtual router for which you want to log events
- remote-ip-address—Logs events for a remote address
- ipAddress—Address of remote system for which you want to log messages
- ipAddressMask—Mask for the remote address