Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Constituent Selection for Shared Shaping Overview
- Implicit Constituent Selection Overview
- scheduler-profile
- shared-shaping-constituent
- shared-shaping-rate

# Configuring Implicit Constituents for Simple or Compound Shared Shaping

There are two types of implicit constituents:

- Simple implicit—Constituents are best-effort node or queues, and all nodes and queues in named traffic-class groups.
- Compound implicit—Constituents are selected automatically by the software. If a node exists in a given traffic-class group, the node is active and the queues stacked above it are inactive constituents.

Before you configure implicit constituents:

- Configure the traffic classes and traffic-class groups.

  See Configuring Traffic Classes That Define Service Levels and Configuring Traffic-Class Groups That Define Service Levels.

To configure implicit constituents:

1. Create the scheduler profile.
   host1(config)#scheduler-profile implicit
2. Configure the shared shaper.

   To configure a simple shared shaper:

   host1(config-scheduler-profile)#shared-shaping-rate 128000 bps

   To configure a compound shared shaper:

   host1(config-scheduler-profile)#shared-shaping-rate 128000 burst 32767 compound
3. (Optional) For compound shared shapers, specify the attributes for the constituent.
   host1(config-scheduler-profile)#shared-shaping-constituent weight 28

   Including this command does not affect how the system selects the compound implicit constituent. If the command is present for a constituent that was implicitly selected, the software configures that constituent using the strict-priority or weight attributes.

After you configure implicit constituents:

- Configure the scheduler hierarchy with the best-effort nodes and queues.

  See Configuring a QoS Profile.

## Related Documentation

- Constituent Selection for Shared Shaping Overview
- Implicit Constituent Selection Overview
- scheduler-profile
- shared-shaping-constituent
- shared-shaping-rate

#### Published: 2011-03-17

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out