# show ip tunnel reassembly statistics

#### Syntax

show ip tunnel reassembly statistics [ detail ] [ all ] [ delta ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
delta keyword added in JunosE Release 8.0.0.

#### Description

Displays statistics on the reassembly of fragmented tunnel packets within the current virtual router context.

#### Options

- detail—Displays detailed reassembly statistics that include packets reassembled or discarded per protocol
- all—Displays reassembly statistics for all virtual routers on the router
- delta—Displays baselined reassembly statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec