# show ip static

#### Syntax

show ip static [ vrfName ] [ ipAddress ipMask [ all ] ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays general status information for static routes added by network management to the routing table.

#### Options

- vrfName—Name of the VRF
- ipAddress—IP address to show
- ipMask—IP mask of the specific address to show
- all—Displays all routes starting at the specified prefix
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec