# Managing SRP Module Redundancy

You can prevent the redundant SRP module from taking over when:

- The primary SRP module experiences a software failure.
- You push the reset button on the primary SRP module.

  | Note: If you do not configure this option, when troubleshooting an SRP module, disconnect the other SRP module from the router. This action prevents the redundant SRP module from taking over if you push the reset button on the primary SRP module.

To configure this option:

1. Issue the disable-switch-on-error command.
   host1(config)#disable-switch-on-error
2. Synchronize the NVS file system of the redundant SRP module to that of the primary SRP module.
   host1#synchronize low-level-check all

#### Related Documentation

- Understanding SRP Module Redundancy
- Installing a Redundant SRP Module
- disable-switch-on-error
- synchronize