# Monitoring LDP Profiles

#### Purpose

Display a specific LDP profile, or all LDP profiles.

#### Action

To display the default LDP profile:

    host1:pe2#show ldp profile default
    ldp profile default: used by 2 interfaces
       session retry:  10 times at interval 10

| Note: The mpls keyword is optional and is provided for compatibility with non–E Series implementations.

#### Meaning

Table 69 lists the show ldp profile command output fields.

Table 69: show ldp profile Output Fields

Field Name | Field Description
--- | ---
profile | Number of interfaces that use the profile
session retry | Number of attempts that will be made to set up an MPLS LDP session

#### Related Documentation

- show ldp profile