# Clearing and Refreshing IPv4 Dynamic Routes in the Tunnel Routing Table

To clear and then refresh a specified IPv4 dynamic route or all IPv4 dynamic routes from the tunnel routing table of the virtual router or a specified VRF:

- Issue the clear ip tunnel-routes command.
  host1(config)#clear ip tunnel-routes *

There is no no version. This command takes effect immediately.

#### Related Documentation

- clear ip tunnel-routes