# show mpls next-hop

#### Syntax

show mpls next-hop [ nextHopIndex ] [ delta ] [ filter ]

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Displays MPLS next hops and any available next-hop statistics. Next hops can be pointed to by MPLS forwarding entries on an LSR, IP or IPv6 routes on an LER, and VPLS bridge groups.

#### Options

- nextHopIndex—Number identifying a next hop, in the range 1–1048575
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec