# show bridge table

#### Syntax

show bridge { bridgeGroupName | vplsName } table [ static | dynamic ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
vplsName variable added in JunosE Release 7.1.0.

#### Description

Displays information about the entries in the MAC address table for the specified bridge group or VPLS instance. You can display information only for static entries, only for dynamic entries, or for both static and dynamic entries.

#### Options

- bridgeGroupName—Name of a bridge group specified with the bridge command
- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command
- static—Displays information for only static (nonlearned) entries in the MAC address table
- dynamic—Displays information for only dynamic (learned) entries in the MAC address table
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Documentation

- Monitoring MAC Address Entries for a Specific VPLS Instance in the JunosE BGP and MPLS Configuration Guide