# baseline bridge

#### Syntax

baseline bridge { bridgeGroupName | vplsName }

#### Release Information

Command introduced before JunosE Release 7.1.0.
vplsName variable added in JunosE Release 7.1.0.

#### Description

Sets a statistics baseline for a bridge group or VPLS instance. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Options

- bridgeGroupName—Name of a bridge group specified with the bridge command
- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command

#### Mode

Privileged Exec

#### Related Documentation

- Setting a Baseline for VPLS Statistics in the JunosE BGP and MPLS Configuration Guide