# sscc restart

#### Syntax

sscc restart [ clean-state ]

#### Release Information

Command introduced in JunosE Release 11.0.0.

#### Description

Forces the router to restart a COPS connection to, and resynchronize with, the SRC software, without removing the SRC client. The no sscc enable cops command removes the SRC client. There is no no version.

#### Options

- clean-state—Enables a complex restart where the SRC client closes the connection and clears the Policy Information Base (PIB) structures and tables. Then the SRC client connects to the SRC software, which requests full synchronization, which restores correct policy and QoS provisioning.

#### Mode

Privileged Exec