# Monitoring DHCP Bindings (Local Server Binding Information)

#### Purpose

Display DHCP local server binding information for DHCP local server clients. Optionally, specify an IP address or an interface to display binding information for a particular address or interface.

| Note: This command is deprecated and might be removed completely in a future release. The function provided by this command has been replaced by the show dhcp binding command.

#### Action

To display DHCP local server binding information for a specific IP address:

    host1#show ip dhcp-local binding 192.168.1.3

                            Dhcp Local Bindings
                            -------------------
      Address         Hardware        Lease      Interface        State
    -----------   -----------------   -----   ----------------   -------
    192.168.1.3   11-11-22-22-33-33   (600)   fastEthernet 5/0   expired

To display DHCP local server binding information for a specific interface:

    host1#show ip dhcp-local binding interface fastethernet 5/0.2

                            Dhcp Local Bindings
                            -------------------
      Address         Hardware        Lease      Interface          State
    -----------   -----------------   -----   ------------------   -------
    192.168.0.6   40-00-00-0b-00-01   240     fastEthernet 5/0.2   bound
    192.168.0.7   40-00-00-0c-00-01   240     fastEthernet 5/0.2   bound
    192.168.1.3   11-11-22-22-33-33   (600)   fastEthernet 5/0.2   expired

#### Meaning

Table 111 lists the show ip dhcp-local binding command output fields.

Table 111: show ip dhcp-local binding Output Fields

Field Name | Field Description
--- | ---
Address | IP address
Hardware | MAC address of subscriber’s computer
Lease | Infinite, or the number of seconds in which the IP address is available; grace period is shown in parentheses for clients in a grace period
Interface | Interface whose statistics are reported
State | Binding state; expired or released state for clients currently in the grace period

#### Related Documentation

- show ip dhcp-local binding