# ipv6 static-route table-map

#### Syntax

ipv6 static-route table-map [ vrf vrfName ] mapName

no ipv6 static-route table-map [ vrf vrfName ] [ mapName ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
vrf keyword and vrfName variable added in JunosE Release 7.2.0.

#### Description

Filters static routes before adding them to the routing table. The no version deletes the table map.

#### Options

- vrfName—Name of the VRF; string of 1–32 alphanumeric characters
- mapName—Name of the table map that you want the router to use

#### Mode

Global Configuration