# Setting the Mask Value for MPLS Rate-Limit Profiles

You can use the exp-mask command to set the mask value used for MPLS rate-limit profiles, in the range 1–255. The no version restores the default value, 7. This command is associated with the committed-action, conformed-action, and exceeded-action commands.

- Issue the exp-mask command from Rate Limit Profile Configuration mode.
  host1(config-rate-limit-profile)#exp-mask 5

#### Related Documentation

- mask-val