# ripGeneral

#### Description

RIP system notifications

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Failed to redistribute an external route to the RIP; failed to establish peer with neighbor due to the memory limitation; general RIP configuration error, such as an access list name or route map name specified in the RIP config mode exceed maximum allowable length

#### Warning Log

Failed to process a RIP packet due to the current memory limitation

#### Notice Log

Enable or disable RIP application

#### Info

None

#### Debug

RIP query; RIP peer address

#### Filter 1

interface interfaceType interfaceSpecifier

- interface—Logs PPP events for a specific interface
- interfaceType—Type of interface for which you want to log events
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JunosE Command Reference Guide.

#### Filter 2

router virtualRouterName

- router—Logs events for a specific virtual router
- virtualRouterName—Name of virtual router for which you want to log events