# Monitoring the Policy Configuration of ATM Subinterfaces

#### Purpose

Display information about a subinterface’s ATM policy lists.

#### Action

To display information about ATM policy lists:

    host1#show atm subinterface
    ATM policy input PolCbr
      classifier-group *
    3096packets, 377678 bytes
    traffic-class best-effort
    color green

#### Meaning

Table 31 lists the show atm subinterface command output fields.

Table 31: show atm subinterface Output Fields

Field Name | Field Description
--- | ---
ATM policy | Type and name of the ATM policy
mark-clp | CLP bit value, 0 or 1
color | Color applied to packet flow for queuing: green, yellow, or red
classifier-group | Name of the classifier control list used by the policy
filter | Filter policy action
forward | Forward policy action
traffic-class | Traffic class in the policy list
user packet class | User packet class in the policy list

#### Related Documentation

- show atm interface