# show l2tp dial-out session

#### Syntax

show l2tp dial-out session [ triggerIpAddress | allVirtualRouters ] [ detail ]
[ state operState ] [ filter ]

To display summary information:

show l2tp dial-out session summary [ allVirtualRouters ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays the status of L2TP dial-out sessions.

#### Options

- triggerIpAddress—Trigger IP address for the session that you want to display
- allVirtualRouters—Displays dial-out information for all virtual routers
- detail—Displays configuration, state, and statistics
- operState—One of the following operational states:
  - authenticating
  - connecting
  - dormant
  - failed
  - inService
  - inhibited
  - pending
  - postInhibited
- filter—See Filtering show Commands
- summary—Displays aggregate counts for dial-out sessions in each of the possible operational and administrative states

#### Mode

Privileged Exec