# mpls ldp graceful-restart recovery-time

#### Syntax

mpls ldp graceful-restart recovery-time [ seconds ]

no mpls ldp graceful-restart recovery-time

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Specifies the length of time the router retains its MPLS forwarding state across a restart. The no version restores the default value, 120 seconds.

#### Options

- seconds—Number of seconds in the range 120–600

#### Mode

Global Configuration