# isis mesh-group

#### Syntax

isis mesh-group { blocked | number }

no isis mesh-group

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures an interface in the same mesh group to act as a virtual multiaccess network. The no version disables the feature.

#### Options

- blocked—Blocks reserved LSPs from being flooded out on this defined configured interface
- number—Mesh group number in the range 1–4294967295

#### Mode

Interface Configuration, Subinterface Configuration