# exception source

#### Syntax

exception source ipAddress ipAddressMask

no exception source

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the IP address and mask of the router interface over which you want to send the core dump file to the remote FTP server. The no version returns the value to its default (null).

#### Options

- ipAddress—IP address of the interface
- ipAddressMask—Optionally add the IP address mask of the interface

#### Mode

Global Configuration