# ipv6 mld immediate-leave

#### Syntax

[ no ] ipv6 mld immediate-leave

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Removes an interface immediately when the router receives a leave group membership message from the host associated with this interface. The no version restores the default situation, in which the router issues query messages to multicast groups and removes an interface if the associated host does not return a group membership report within a certain length of time.

| Caution: Issue this command only on MLDv1 interfaces to which one MLD client is connected. Do not issue this command to interfaces to which more than one MLD client is connected.

#### Mode

Interface Configuration, Profile Configuration