# service dhcp-local

#### Syntax

[ no ] service dhcp-local [ equal-access | standalone [ authenticate ] ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables the DHCP local server. In standalone mode, the authenticate keyword enables AAA-based authentication for incoming DHCP clients. The no version disables the DHCP local server and does not save the previous settings.

#### Options

- equal-access—Enables the DHCP local server to work with the SRC (formerly SDX or SSC) or HTTP local server for non-PPP equal access, the default option
- standalone—Configures the router as a DHCP local server
- authenticate—Enables AAA-based authentication of incoming DHCP clients

#### Mode

Global Configuration