# Monitoring RADIUS Dynamic-Request Server Statistics

#### Purpose

Display RADIUS dynamic-request server statistics.

#### Action

To display RADIUS dynamic-request statistics:

    host1#show radius dynamic-request statistics

           RADIUS Request Statistics
           -------------------------
              Statistic             10.10.3.4
    -----------------------------   -------
    UDP Port                        1700
    Disconnect Requests             0
    Disconnect Accepts              0
    Disconnect Rejects              0
    Disconnect No Session ID        0
    Disconnect Bad Authenticators   0
    Disconnect Packets Dropped      0
    CoA Requests                    0
    CoA Accepts                     0
    CoA Rejects                     0
    CoA No Session ID               0
    CoA Bad Authenticators          0
    CoA Packets Dropped             0
    No Secret                       0
    Unknown Request                 0

    Invalid Addresses Received  :0

#### Meaning

Table 61 lists the show radius dynamic-request statistics command output fields.

Table 61: show radius dynamic-request statistics Output Fields

Field Name | Field Description
--- | ---
Udp Port | Port on which the router listens for RADIUS server
Disconnect or CoA Requests | RADIUS-initiated disconnect or CoA requests received
Disconnect or CoA Accepts | RADIUS-initiated disconnect or CoA requests accepted
Disconnect or CoA Rejects | RADIUS-initiated disconnect or CoA requests rejected
Disconnect or CoA No Session ID | RADIUS-initiated disconnect or CoA messages rejected because the request did not include a session ID attribute
Disconnect or CoA Bad Authenticators | RADIUS-initiated disconnect or CoA messages rejected because the calculated authenticator in the authenticator field of the request did not match
Disconnect or CoA Packets Dropped | RADIUS-initiated disconnect or CoA packets dropped because of queue overflow
No Secret | Messages rejected because a secret was not present in the authenticator field
Unknown Requests | Packets received with an invalid RADIUS code for RADIUS disconnect or change of authorization
Invalid Addresses Received | Number of invalid addresses received

#### Related Documentation

- Setting the Baseline for RADIUS Dynamic-Request Server Statistics
- show radius statistics