# baseline ip tunnel-reassembly

#### Syntax

baseline ip tunnel-reassembly

#### Release Information

Command introduced in JunosE Release 8.0.0.

#### Description

Sets a statistics baseline for tunnel reassembly statistics on the current virtual router. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever you retrieve baseline-relative statistics. There is no no version.

#### Mode

Privileged Exec